2004/08/10 MKH


'BIN' folder contains executable example programs. Planmeca dlls and decive drivers are needed for completing
a run-time environment. See 'SETUP' for installation of the dlls and drivers.  
VBDidapiUI.exe needs VB6.0 run time components. See 'Demoimages' folder for explanation
of enabling simulated image grabbing.

'Demoimages' folder contains demo images that are needed for image grabbing simulation.
If the images are copied to 'BIN' folder, no Planmeca devices are needed for testing
image capturing. Real image grabbing needs installation of Planmeca device drivers and 
device. See 'Setup' folder explanation. 


'DidapiUI' folder contains model description of the new DidapiUI 
library (= the new function 'DUI_capture_image_ex()' function).

'DidapiUI_old' folder contains a VC++ 6.0 libary project. Only one function call is needed
for image capturing with this library. That function ('DUI_capture_image()') calls all necessary 
didapi.dll functions that are needed for grabbing an image.

'DOCS' contains DIDAPI, DidapiUI, DidapiUIsample DidapiUI Twain source documents.

'INCLUDE' folder contains header file of didapi and didapiUI libraries.

'LIB' folder contains 'didapi.lib' library file.

'SETUP' folder contains Planmeca device driver installation package.
The drivers are compatible with Dimaxis Pro 3.2.3 version, but Dimaxis installation
is not needed for image capturing if the device drivers have been installed with
this setup. Setup program installs drivers into windows driver folder and Planmeca dlls
into user selected folder, also if the path is given as a parameter to the setup.exe program.
The path is added into Windows PATH environment string. 

'VBdidapiUI_old sample' and 'VCdidapiUI_old sample' folders contain VB6.0 and VC++6.0 example
project source codes. They use wrapper libary 'DidapiUI.dll' that use 'didapi.dll'
library. The old library function is called.

'Twain Source' folder contains documents and information about the Planmeca DidapiUI Twain source
implementation.   