; Installation INF for the USB2.0 Driver for Windows XP/VISTA 64-bit
; Version 3.0.0.02

[Version]
Signature="$WINDOWS NT$"
Class=USB
ClassGUID                = {36FC9E60-C465-11CF-8056-444553540000}
provider                 = %PROVIDER%
DriverPackageType        = PlugAndPlay
DriverPackageDisplayName = %USBHS64_Package%
DriverVer                = 01/06/2010,3.0.0.02
CatalogFile              = usbhs20_64bit.cat

[SourceDisksNames]
1=%USBHS64_INSTALL%,,,

[SourceDisksFiles]
USBHS64.sys = 1

[DestinationDirs]
USBHS64.Files.Ext = 10,System32\Drivers

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%USBHS64_Provider%=Device,NT,NTx86,NTamd64

;for all platforms
[Device]
%VID_082e&PID_1005.DeviceDesc%=USBHS64, USB\VID_082e&PID_1005


;for windows 2000 non intel platforms
[Device.NT]


;for x86 platforms
[Device.NTx86]


;for x64 platforms
[Device.NTamd64]
%VID_082e&PID_1005.DeviceDesc%=USBHS64, USB\VID_082e&PID_1005
%VID_082E&PID_2000.DeviceDesc%=USBHS64, USB\VID_082E&PID_2000


[USBHS64]
CopyFiles=USBHS64.Files.Ext
AddReg=USBHS64.AddReg

[USBHS64.HW]
AddReg=USBHS64.AddReg.Guid

[USBHS64.Services]
Addservice = USBHS64,2,USBHS64.AddService

[USBHS64.NT]
CopyFiles=USBHS64.Files.Ext
AddReg=USBHS64.AddReg

[USBHS64.NT.HW]
AddReg=USBHS64.AddReg.Guid

[USBHS64.NT.Services]
Addservice = USBHS64,2,USBHS64.AddService


[USBHS64.NTx86]
CopyFiles=USBHS64.Files.Ext
AddReg=USBHS64.AddReg

[USBHS64.NTx86.HW]
AddReg=USBHS64.AddReg.Guid

[USBHS64.NTx86.Services]
Addservice = USBHS64,2,USBHS64.AddService

[USBHS64.NTamd64]
CopyFiles=USBHS64.Files.Ext
AddReg=USBHS64.AddReg

[USBHS64.NTamd64.HW]
AddReg=USBHS64.AddReg.Guid

[USBHS64.NTamd64.Services]
Addservice = USBHS64,2,USBHS64.AddService


[USBHS64.AddReg]

HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,USBHS64.sys

HKR,,DriverBase,,USBHS64.sys
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2
HKR,,FriendlyName,,%USBHS64_Description%

[USBHS64.AddService]
DisplayName    = %USBHS64_Description%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\USBHS64.sys
AddReg         = USBHS64.AddReg
LoadOrderGroup = Base

[USBHS64.Files.Ext]
USBHS64.sys

[USBHS64.AddReg.Guid]
HKR,,DriverGUID,,%USBHS64.GUID%

[Strings]
PROVIDER            = "SDR Manufacturer"
USBHS64_Provider    = "SDR Manufacturer"
USBHS64_Company     = "SDR Manufacturer"
USBHS64_Description = "SDR Generic USB Driver"
USBHS64_DisplayName = "SDR USB Generic"
USBHS64_INSTALL     = "USB 2.0 Generic EZ-USB Driver Installation Disk"
USBHS64_Package     = "Digital Radiography Device"
USBHS64.GUID        = "{A286F2AA-354D-4131-8129-038F49CB0161}"
USBHS64_Unused      = "."

VID_082e&PID_2000.DeviceDesc="Digital Radiography Device (SDR2000 A)"
VID_082e&PID_1005.DeviceDesc="Digital Radiography Device (SDR303 A)"
